Drift Scan (TDI) scanning pattern during 6 months

±π/4 solar acceptance ±π/8 solar acceptance (12% loss)

N_f shuttle motions

10*N_{filter} shuttle motions 12*Nfilter shuttle motions

E.B. 12 mai 2005